Pattern has four layers

Each layer has either note CV or mod CV plus a single gate lane

Note CV

* Note name guide on screen when setting note
* 1V/octave
* Outputs MIDI note

Mod CV

* Voltage range can be set
* Outputs MIDI CC or MIDI velocity when paired with another note track